Valve JZ has flow rate=0; tunnels lead to valves IR, LY
Valve KD has flow rate=0; tunnels lead to valves NJ, ZS
Valve VW has flow rate=0; tunnels lead to valves IT, VH
Valve HS has flow rate=0; tunnels lead to valves OC, PN
Valve EU has flow rate=19; tunnel leads to valve GQ
Valve XF has flow rate=0; tunnels lead to valves WL, QD
Valve DD has flow rate=8; tunnels lead to valves GQ, YY, JV, SK
Valve TA has flow rate=0; tunnels lead to valves NJ, VJ
Valve IR has flow rate=9; tunnels lead to valves JZ, WI, VJ, GC, WG
Valve SS has flow rate=17; tunnels lead to valves SI, IZ, RK, WI
Valve SG has flow rate=0; tunnels lead to valves NV, NJ
Valve IT has flow rate=0; tunnels lead to valves LL, VW
Valve CP has flow rate=24; tunnels lead to valves HN, ZK, EJ
Valve SK has flow rate=0; tunnels lead to valves LL, DD
Valve IS has flow rate=0; tunnels lead to valves AA, LL
Valve HN has flow rate=0; tunnels lead to valves FF, CP
Valve VH has flow rate=10; tunnels lead to valves QO, VW, RV, PN
Valve JV has flow rate=0; tunnels lead to valves DD, RK
Valve ZS has flow rate=0; tunnels lead to valves KD, LL
Valve UC has flow rate=25; tunnels lead to valves JD, IV
Valve WI has flow rate=0; tunnels lead to valves SS, IR
Valve UR has flow rate=0; tunnels lead to valves QD, LY
Valve GC has flow rate=0; tunnels lead to valves AA, IR
Valve YY has flow rate=0; tunnels lead to valves DD, AA
Valve IV has flow rate=0; tunnels lead to valves ZK, UC
Valve BM has flow rate=0; tunnels lead to valves SA, WL
Valve JD has flow rate=0; tunnels lead to valves IZ, UC
Valve WL has flow rate=12; tunnels lead to valves EF, BM, EJ, XF
Valve AA has flow rate=0; tunnels lead to valves NV, YY, GC, IS, QO
Valve WG has flow rate=0; tunnels lead to valves LL, IR
Valve GQ has flow rate=0; tunnels lead to valves EU, DD
Valve SI has flow rate=0; tunnels lead to valves SS, NJ
Valve KH has flow rate=13; tunnels lead to valves SA, ON
Valve PC has flow rate=22; tunnel leads to valve ON
Valve QD has flow rate=14; tunnels lead to valves XF, UR
Valve IZ has flow rate=0; tunnels lead to valves SS, JD
Valve QO has flow rate=0; tunnels lead to valves AA, VH
Valve SA has flow rate=0; tunnels lead to valves BM, KH
Valve NV has flow rate=0; tunnels lead to valves AA, SG
Valve ZK has flow rate=0; tunnels lead to valves CP, IV
Valve ON has flow rate=0; tunnels lead to valves PC, KH
Valve PN has flow rate=0; tunnels lead to valves HS, VH
Valve RV has flow rate=0; tunnels lead to valves NJ, VH
Valve RK has flow rate=0; tunnels lead to valves SS, JV
Valve OC has flow rate=18; tunnel leads to valve HS
Valve EF has flow rate=0; tunnels lead to valves LY, WL
Valve VJ has flow rate=0; tunnels lead to valves TA, IR
Valve LL has flow rate=5; tunnels lead to valves ZS, IT, SK, IS, WG
Valve FF has flow rate=0; tunnels lead to valves HN, LY
Valve LY has flow rate=21; tunnels lead to valves EF, FF, UR, JZ
Valve EJ has flow rate=0; tunnels lead to valves WL, CP
Valve NJ has flow rate=6; tunnels lead to valves RV, KD, SG, SI, TA
